{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["室内试验"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"室内试验","index":0,"n_rows":88,"n_cols":10,"rows_kept":88,"merged":[[1,0,2,9],[1,10,2,11],[3,0,3,9],[4,2,4,3],[5,0,18,0],[5,1,6,1],[5,2,5,3],[6,2,6,3],[7,1,12,1],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,1,17,1],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,0,22,0],[19,1,22,1],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,0,32,0],[23,1,29,1],[23,2,23,3],[24,2,24,3],[25,2,25,3],[26,2,26,3],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,1,32,1],[30,2,30,3],[31,2,31,3],[32,2,32,3],[33,0,50,0],[33,1,36,1],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,1,43,1],[37,2,37,3],[38,2,38,3],[39,2,39,3],[40,2,40,3],[41,2,41,3],[42,2,42,3],[43,2,43,3],[44,1,50,1],[44,2,44,3],[45,2,45,3],[46,2,46,3],[47,2,47,3],[48,2,48,3],[49,2,49,3],[50,2,50,3],[51,0,68,0],[51,1,55,1],[51,2,53,2],[54,2,54,3],[55,2,55,3],[56,1,59,1],[56,2,56,3],[57,2,57,3],[58,2,58,3],[59,2,59,3],[60,1,68,1],[60,2,60,3],[61,2,61,3],[62,2,62,3],[63,2,63,3],[64,2,64,3],[65,2,65,3],[66,2,66,3],[67,2,67,3],[68,2,68,3],[69,0,83,0],[69,2,69,3],[70,1,72,1],[70,2,70,3],[71,2,71,3],[72,2,72,3],[73,1,75,1],[73,2,73,3],[74,2,74,3],[75,2,75,3],[76,1,79,1],[76,2,76,3],[77,2,77,3],[78,2,78,3],[79,2,79,3],[80,1,83,1],[80,2,80,3],[81,2,81,3],[82,2,82,3],[83,2,83,3],[84,0,86,0],[84,1,86,1],[84,2,84,3],[85,2,85,3],[86,2,86,3],[87,0,87,6],[87,8,87,9]],"flags":["formulas_cached_only"]}
["附件2"]
["长春绕城高速公路2020年养护专项工程试验检测项目清单"]
[]
["检测单位名称（专用章）：  "]
["工程名称","材料名称","检测项目",null,"单位","分项标准单价（元）","抽检频率或数量","检测收费金额（元）","自检频率","备注"]
["桥梁工程","砼","抗压强度",null,"组"]
[null,null,"抗冻性",null,"项"]
[null,"钢筋","质量偏差",null,"项"]
[null,null,"屈服强度",null,"项"]
[null,null,"抗拉强度",null,"项"]
[null,null,"伸长率",null,"项"]
[null,null,"冷弯试验",null,"项"]
[null,null,"反向弯曲",null,"项"]
[null,"水泥混凝土配合比","C类配合比验证",null,"项"]
[null,"伸缩缝橡胶","拉伸试验",null,"项"]
[null,null,"热空气老化试验",null,"项"]
[null,null,"耐盐水性试验",null,"项"]
[null,null,"耐油污性试验",null,"项"]
[null,"砂浆","抗压强度",null,"组"]
["沥青混凝土路面","粗集料","筛分",null,"项"]
[null,null,"针片状",null,"项"]
[null,null,"＜0.075mm 颗粒含量",null,"项"]
[null,null,"压碎值",null,"项"]
["沥青混凝土路面","粗集料","软石含量",null,"项"]
[null,null,"表观相对密度",null,"项"]
[null,null,"吸水率",null,"项"]
[null,null,"粘附性",null,"项"]
[null,null,"坚固性",null,"项"]
[null,null,"洛杉矶磨耗",null,"项"]
[null,null,"磨光值",null,"项"]
[null,"细集料","筛分",null,"项"]
[null,null,"＜0.075mm 含量",null,"项"]
[null,null,"砂当量",null,"项"]
["沥青混凝土路面","细集料","亚甲兰值",null,"项"]
[null,null,"棱角性",null,"项"]
[null,null,"表观密度",null,"项"]
[null,null,"坚固性",null,"项"]
[null,"矿粉","表观密度",null,"项"]
[null,null,"含水量",null,"项"]
[null,null,"筛分",null,"项"]
[null,null,"外观",null,"项"]
[null,null,"亲水系数",null,"项"]
[null,null,"塑性指数",null,"项"]
[null,null,"加热安定性",null,"项"]
[null,"改性沥青","针入度",null,"项"]
[null,null,"延度",null,"项"]
[null,null,"软化点",null,"项"]
[null,null,"贮存稳定性离析",null,"项"]
[null,null,"针入度指数PI",null,"项"]
[null,null,"运动粘度（135℃）",null,"项"]
[null,null,"弹性恢复",null,"项"]
["沥青混凝土路面","改性沥青","TFOT（或RTFOT）后","质量变化","项"]
[{"$nulls":3},"针入度比   （25℃）","项"]
[{"$nulls":3},"延度 （5℃）","项"]
[null,null,"闪点",null,"项"]
[null,null,"溶解度",null,"项"]
[null,"应力吸收层橡胶沥青","运动粘度（180-190℃）",null,"项"]
[null,null,"针入度",null,"项"]
[null,null,"软化点",null,"项"]
[null,null,"弹性恢复",null,"项"]
[null,"改性乳化沥青","蒸发残留物含量",null,"项"]
[null,null,"蒸发残留物针入度",null,"项"]
[null,null,"蒸发残留物软化点",null,"项"]
[null,null,"蒸发残留物延度",null,"项"]
[null,null,"蒸发残留物溶解度",null,"项"]
[null,null,"蒸发残留物弹性恢复",null,"项"]
[null,null,"常温贮存稳定性",null,"项"]
[null,null,"1.18mm筛上剩余量",null,"项"]
[null,null,"粘度",null,"项"]
["沥青混凝土路面","改性乳化沥青","与粗集料粘附性",null,"项"]
[null,"木质素纤维","筛分析",null,"项"]
[null,null,"纤维长度",null,"项"]
[null,null,"灰分含量",null,"项"]
[null,"木质素纤维","PH值",null,"项"]
[null,null,"吸油率",null,"项"]
[null,null,"含水量",null,"项"]
[null,"沥青混合料","沥青含量试验",null,"项"]
[null,null,"级配",null,"项"]
[null,null,"马歇尔稳定度试验",null,"组"]
[null,null,"最大理论密度试验",null,"项"]
[null,"沥青混合料","车辙试验",null,"组"]
[null,null,"残留稳定度试验",null,"组"]
[null,null,"析漏试验",null,"项"]
[null,null,"飞散试验",null,"项"]
["沥青混凝土路面","沥青混合料","冻融劈裂强度试验",null,"项"]
[null,null,"低温弯曲试验",null,"项"]
[null,null,"沥青混凝土配合比（委托）验证检测",null,"项"]
["总合计"]